BLIND SPOT MONITORING (BSM) INDICATOR LIGHT CONSTRUCTION/OPERATION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE]

id0922009982e1

• Equipped in the left and right outer mirror glasses.
• LEDs with low-power consumption and high durability have been adopted.
• Illuminates for approx. 3 s after the ignition switch is turned to the ON position to perform a bulb check.
• If a vehicle enters the alert area, illuminates or flashes according to the signal from the BSM control module to alert or warn the driver.
• Refer to BLIND SPOT MONITORING (BSM) OPERATION for the illumination/flash conditions of the BSM indicator light. (See BLIND SPOT MONITORING (BSM) OPERATION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)