FRONT BUMPER REMOVAL/INSTALLATION

id091000800300

1. Disconnect the negative battery cable.

2. Remove the clip of the front over fender and put aside the front bumper.

ac9uuw00002345

3. Remove in the order indicated in the table.

ac9uuw00004634

1 | Screw A
2 | Bolt
3 | Fastener A
4 | Fastener B
5 | Screw B
6 | Front bumper (See Front Bumper Removal Note) (See Front Bumper Installation Note)

4. Disconnect the front fog light connector. (Vehicles with front fog lights)

5. Install in the reverse order of removal.

6. Adjust the front fog light aiming for vehicles with front fog lights. (See FRONT FOG LIGHT AIMING.)

Front Bumper Removal Note

1. Pull the front bumper ends (wheel arch) outward (1) to disengage from the bumper slider.

ac9uuw00004635

  Caution
  • When disengaging the front bumper from the bumper slider, the front bumper could fall and be damaged. Secure the front bumper so that it does not fall.

2. Remove the front bumper from the body.

Front Bumper Installation Note

1. Spread the front bumper ends apart.

2. Assemble the front bumper to the body.

3. Press the front bumper connecting area into the body to engage with the bumper slider.