BLIND SPOT MONITORING (BSM) CONTROL MODULE REMOVAL/INSTALLATION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE]

id0922008100e2

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

2. Remove the rear combination light. (See REAR COMBINATION LIGHT REMOVAL/INSTALLATION.)

3. Remove the rear bumper. (See REAR BUMPER REMOVAL/INSTALLATION.)

4. Disconnect the connector.

ac9uuw00004938

5. Remove the nuts.

6. Remove the BSM control module.

7. Install in the reverse order of removal.

8. Perform the blind spot monitoring radar test. (See BLIND SPOT MONITORING (BSM) RADAR TEST [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)

  Caution
  • If the BSM control module is replaced, not performing the BSM radar test will cause a deviation in the radar emission angle which could result in the system not detecting a vehicle approaching from the rear correctly. If the BSM control module is replaced, perform the BSM radar test.