FRONT BLOWER MOTOR REMOVAL/INSTALLATION

id074000805000

1. Disconnect the negative battery cable.

2. Remove the dashboard under cover. (passenger side) (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

L.H.D.

ac9wzw00002811

R.H.D.

ac9wzw00002812

1 | Front blower motor connector
2 | Screw
3 | Front blower motor

4. Install in the reverse order of removal.