DTC TABLE [THEFT-DETERRENT SYSTEM]

id0902g7960500

DTC | Description | Reference
--- | --- | ---
M-MDS display
B109F:49 | Intruder sensor internal malfunction | (See DTC B109F:49 [THEFT-DETERRENT SYSTEM].)
B109F:86 | Signal error from intruder sensor | (See DTC B109F:86 [THEFT-DETERRENT SYSTEM].)
B109F:87 | Communication error between intruder sensor and theft-deterrent control module | (See DTC B109F:87 [THEFT-DETERRENT SYSTEM].)
B10A5:49 | Theft-deterrent siren internal malfunction | (See DTC B10A5:49 [THEFT-DETERRENT SYSTEM].)
B10A5:86 | Signal error from theft-deterrent siren | (See DTC B10A5:86 [THEFT-DETERRENT SYSTEM].)
B10A5:87 | Communication error between theft-deterrent siren and theft-deterrent control module | (See DTC B10A5:87 [THEFT-DETERRENT SYSTEM].)
B1174:13 | Door lock-link switch (passenger-side/LR/RR) circuit malfunction | (See DTC B1174:13 [THEFT-DETERRENT SYSTEM].)
P254F:13 | Bonnet latch switch circuit malfunction | (See DTC P254F:13 [THEFT-DETERRENT SYSTEM].)
U0001:88 | Module communication error (HS-CAN) | (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0100:00 | Communication error with PCM
U0300:00 | Possible configuration error | (See DTC U0300:00, U2100:00, [THEFT-DETERRENT SYSTEM].)
U2100:00
U3000:49 | Theft-deterrent control module internal malfunction | (See DTC U3000:49 [THEFT-DETERRENT SYSTEM].)
U3003:16 | Theft-deterrent control module power supply circuit malfunction | (See DTC U3003:16, U3003:17 [THEFT-DETERRENT SYSTEM].)
U3003:17