DTC TABLE [FORWARD SENSING CAMERA (FSC)]

id0902p9029400

×: Applicable
—: Not applicable

DTC No. | HBC warning light (amber) | “ERROR” in LCD display | Detection condition | Description | Fail-safe function | Drive cycle | Self test type*1 | Memory function | Page
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
B115E:54 | Flash | × | • Forward sensing camera (FSC) aiming not completed is detected. | Forward sensing camera (FSC) aiming not completed | × | — | C, D | × | (See DTC B115E:54 [FORWARD SENSING CAMERA (FSC)].)
B13A6:11 | — | × | • Forward sensing camera (FSC) detects that the FOW/LDWS switch is held pressed for 30 s or more. | FOW/LDWS switch circuit malfunction | × | — | C, D | × | (See DTC B13A6:11 [FORWARD SENSING CAMERA (FSC)].)
C1001:92 | Illuminate | × | • With the LDWS switch on or the high beam control (HBC) system or forward obstruction warning (FOW) system operating, it is detected that the area around the forward sensing camera (FSC) is excessively bright, and the system is inoperable for 10 min. | Forward sensing camera (FSC) poor functioning | × | — | C, D | × | (See DTC C1001:92 [FORWARD SENSING CAMERA (FSC)].)
C1001:97 | Illuminate | × | • With the LDWS switch on or the high beam control (HBC) system or forward obstruction warning (FOW) system operating, it is detected that the forward sensing camera (FSC) field of view is obstructed for 10 min. | Forward sensing camera (FSC) poor visibility | × | — | C, D | × | (See DTC C1001:97 [FORWARD SENSING CAMERA (FSC)].)
U0001:88 | Flash | × | • Forward sensing camera (FSC) cannot receive the CAN bus communication signal (HS-CAN) for 1 s or more. • Forward sensing camera (FSC) detects the CAN bus communication line (HS-CAN) malfunction 10 times continuously. | Module communication error (HS-CAN) | × | — | C, D | × | (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].) (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (R.H.D.)].)
U0100:00 | Flash | × | • Forward sensing camera (FSC) cannot receive the CAN signal from the PCM for 1 s or more. | Communication error with PCM | × | — | C, D | ×
U0121:00 | Flash | × | • Forward sensing camera (FSC) cannot receive the CAN signal from the DSC/RSC HU/CM for 1 s or more. | Communication error with DSC/RSC HU/CM | × | — | C, D | ×
U0140:00 | Flash | × | • Forward sensing camera (FSC) cannot receive the CAN signal from the BCM for 5 s or more. | Communication error with BCM | × | — | C, D | ×
U0155:00 | Flash | × | • Forward sensing camera (FSC) cannot receive the CAN signal from the instrument cluster for 5 s or more. | Communication error with instrument cluster | × | — | C, D | ×
U0401:68 | Flash | × | • Forward sensing camera (FSC) receives the error signal from the PCM for 1 s or more. | Error signal from PCM | × | — | C, D | × | (See DTC U0401:68 [FORWARD SENSING CAMERA (FSC)].)
U0415:68 | Flash | × | • Forward sensing camera (FSC) receives the error signal from the DSC/RSC HU/CM for 1 s or more. | Error signal from DSC/RSC HU/CM | × | — | C, D | × | (See DTC U0415:68 [FORWARD SENSING CAMERA (FSC)].)
U0422:68 | Flash | × | • Forward sensing camera (FSC) receives the error signal from the BCM for 5 s or more. | Error signal from BCM | × | — | C, D | × | (See DTC U0422:68 [FORWARD SENSING CAMERA (FSC)].)
U0423:68 | — | × | • Forward sensing camera (FSC) receives the error signal from the instrument cluster for 5 s or more. | Error signal from instrument cluster | × | — | C, D | × | (See DTC U0423:68 [FORWARD SENSING CAMERA (FSC)].)
U2005:86 | Flash | × | • Forward sensing camera (FSC) receives the vehicle speed signal error from the PCM. | Error signal from PCM | × | — | C, D | × | (See DTC U2005:86 [FORWARD SENSING CAMERA (FSC)].)
U2100:00 | Illuminate | × | • Forward sensing camera (FSC) configuration not completed is detected. | Forward sensing camera (FSC) configuration error | × | — | C, D | × | (See DTC U2100:00 [FORWARD SENSING CAMERA (FSC)].)
U2101:00 | Flash | × | • Forward sensing camera (FSC) detects that the forward sensing camera (FSC) has unsupported configuration data. | Forward sensing camera (FSC) configuration error | × | — | C, D | × | (See DTC U2101:00 [FORWARD SENSING CAMERA (FSC)].)
U3000:04 | Flash | × | • Forward sensing camera (FSC) detects the error in the image-related circuit in the forward sensing camera (FSC). | Forward sensing camera (FSC) internal malfunction | × | — | C, D | × | (See DTC U3000:04/U3000:09/U3000:42/U3000:49 [FORWARD SENSING CAMERA (FSC)].)
U3000:09 | Flash | × | • Forward sensing camera (FSC) detects the internal temperature sensor malfunction in the forward sensing camera (FSC). | Forward sensing camera (FSC) internal malfunction | × | — | C, D | ×
U3000:42 | Flash | × | • Forward sensing camera (FSC) detects the NVRAM error in the forward sensing camera (FSC). | Forward sensing camera (FSC) internal malfunction | × | — | C, D | ×
U3000:49 | Flash | × | • Forward sensing camera (FSC) detects the malfunction in the forward sensing camera (FSC). | Forward sensing camera (FSC) internal malfunction | × | — | C, D | ×
U3003:16 | Flash | × | • Forward sensing camera (FSC) power supply circuit voltage is less than 7.2 V for 5 s or more. | Forward sensing camera (FSC) power supply voltage low input | × | — | C, D | × | (See DTC U3003:16 [FORWARD SENSING CAMERA (FSC)].)
U3003:17 | Flash | × | • Forward sensing camera (FSC) power supply circuit voltage is 16.8 V or more for 5 s or more. | Forward sensing camera (FSC) power supply voltage high input | × | — | C, D | × | (See DTC U3003:17 [FORWARD SENSING CAMERA (FSC)].)

*1 :C: CMDTC self test, D: ODDTC self test