FRONT SIDE FRAME (PARTIAL CUTTING) REMOVAL [PANEL REPLACEMENT]

id098008742100

RH

  Caution
  • The rough cut area indicates the maximum size range of the installation position.

1. Rough cut area (A), drill the 19 locations indicated by (B), and then remove the front side frame.

ac9uub00000093

LH

  Caution
  • The rough cut area indicates the maximum size range of the installation position.

1. Rough cut area (A), drill the 19 locations indicated by (B), and then remove the front side frame.

ac9uub00000094