OIL SEAL (MANUAL SHAFT) REPLACEMENT [AY6A-EL, AY6AX-EL]

id0517k3331300

  Caution
  • Water or foreign material entering the connector can cause a poor connection or corrosion. Be sure not to allow water or foreign material on the connector when disconnecting.

1. Disconnect the negative battery cable.

2. Remove the fresh-air duct and air cleaner component as a single unit. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZI-3.7].)

3. Remove the TCM. (See TCM REMOVAL/INSTALLATION [AY6A-EL, AY6AX-EL].)

4. Remove and discard the oil seal using a tape-wrapped flathead screwdriver.

am6xuw00004125

  Caution
  • Do not damage the transaxle case.
  • Do not damage the manual shaft.

5. Using the SSTs and a hammer, tap a new oil seal so that the specified oil seal position is obtained.

am6xuw00004126

  Caution
  • Do not damage the oil seal.

6. Install the TCM. (See TCM REMOVAL/INSTALLATION [AY6A-EL, AY6AX-EL].)

7. Install the fresh-air duct and air cleaner component as a single unit. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZI-3.7].)

8. Connect the negative battery cable.

9. Perform the “TCM NEUTRAL POSITION LEARNING”. (See TCM NEUTRAL POSITION LEARNING [AY6A-EL, AY6AX-EL].)