FRONT DOOR REMOVAL/INSTALLATION

id091100520100

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

ac9uuw00003061

1 | Connector (See Connector Removal Note.)
2 | Bolt A
3 | Bolt B
4 | Front door

3. Install in the reverse order of removal.

4. Adjust the front door. (See DOOR ADJUSTMENT.)

Connector Removal Note

1. Pull down the lever in the direction of the arrow (1) and disconnect the connector in the direction of the arrow (2).

ac9wzw00001192