DTC TABLE [AUDIO]

id0902f6855700

  Note
  • There are two types of procedures for the audio unit inspection; one using the M-MDS and the other which does not (on-board diagnostic test mode). Because the DTCs differ if using or not using the M-MDS, perform the DTC inspection using the M-MDS method and the method not using it. (See DTC INSPECTION [AUDIO].)

× :Applicable
— :Not applicable

DTC | Security indicator light | Description | Fail-safe | Drive cycle | Self-test type*1 | Memory function | Reference
--- | --- | --- | --- | --- | --- | --- | ---
Method using M-MDS | On-board diagnostic test mode
B1188:64 | 10:Er07 | — | Audio unit internal malfunction | — | — | C,D | × | (See DTC: B1188:64, 10:Er07 [AUDIO].)
B1D19:71 | 10:Er02 | — | Audio unit internal malfunction | — | — | C,D | × | (See DTC: B1D19:71, 10:ER02 [AUDIO].)
B1D19:79 | 10:Er01 | — | Audio unit internal malfunction | — | — | C,D | × | (See DTC: B1D19:79, 10:Er01 [AUDIO].)
B1D19:96 | 10:Er10 | — | Audio unit internal malfunction | — | — | C,D | × | (See DTC: B1D19:96, 10:Er10 [AUDIO].)
U0010:88 | 16:Er12 | — | CAN system communication error | — | — | C,D | × | (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].) (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (R.H.D.)].)
U0197:00 | —*2 | — | Communication error with audio unit | — | — | C,D | × | (See DTC: U0197:00, 26:Er81 [Bluetooth SYSTEM (HANDS-FREE TELEPHONE (HF/TEL) SYSTEM)].)
U3000:04 | 09:Er22 | — | Audio unit internal malfunction | × | — | C,D | × | (See DTC: U3000:04, 09:Er22 [AUDIO].)
U3000:09 | 09:Er21 | — | Audio unit internal malfunction | × | — | C,D | × | (See DTC: U3000:09, 09:Er21 [AUDIO].)
U3003:16 | 09:Er20 | — | Voltage decrease input from battery | — | — | C,D | × | (See DTC: U3003:16, 09:Er20 [AUDIO].)
— | —*2 | — | DTCs not stored | — | — | — | — | —

*1 :C: CMDTC self test, D: ODDTC self test
*2 :It is not displayed in the audio display because the on-board diagnostic test mode is not available.