PID/DATA MONITOR TABLE [ADVANCED KEYLESS ENTRY AND START SYSTEM]

id09021g345900

PID/data monitor table

PID name (definition) | Data contents | Unit/Operation | Keyless control module terminal
--- | --- | --- | ---
BUZZER | Keyless beeper | Off/On | 2K
DRSW_ALL | Door switch (all doors) | CLOSE/OPEN | 3Q
DRSW_D | Door switch (driver door) | CLOSE/OPEN | 3Q
DTC_CNT | Number of continuous DTCs | − | −
IG_KEY_IN | Key reminder switch | Key-Out/Key-In | 3F
IG_SW_ST | Ignition switch (Push switch) | Not Pushed/Pushed | 3E
IMMOBI | Immobilizer system equipped or not | Off/On | −
LOCK_SW_D | Door lock-link switch (driver side) | Off/On | 3N
NUMCARD | Number of programmed card keys | − | −
NUMKEY | Number of programmed key ID numbers | − | −
PWR_ACC | Power supply (ACC) | Off/On | 2E
PWR_IG1 | Power supply (IG1) | Off/On | 2C
REQ_SW_BK | Request switch (liftgate) | Off/On | 3M
REQ_SW_D | Request switch (driver door) | Off/On | 3I
REQ_SW_P | Request switch (passenger door) | Off/On | 3K
RPM | Engine speed | RPM | 3W, 3X
TR/LG_SW | Trunk compartment light switch | CLOSE/OPEN | 3P
VPWR | Supply voltage | V | 2A
VSS | Vehicle speed | KPH (MPH) | 3W, 3X

Active command mode table

Command name | Output part name | Unit/Operation | Keyless control module terminal
--- | --- | --- | ---
BZR_INN | Interior buzzer (Instrument cluster) | Off/On | 3W, 3X
BZR_OUT | Keyless beeper | Off/On | 2K
DR_LOCK | All doors lock | Off/Lock | 3Q
DR_UNLOCK | All doors unlock | Off/Unlock | 3Q
LNP_GREEN | Keyless indicator light (green) | Off/On | 3W, 3X
LNP_RED | Keyless warning light (red) | Off/On | 3W, 3X