No.4 SOME DOOR GLASS DO NOT OPERATE [POWER WINDOW SYSTEMS (EXTERIOR OPEN/CLOSE FUNCTION)]

id090361808900

4 | Some door glass do not operate
POSSIBLE CAUSE | • Power window subswitch malfunction • Power window motor malfunction • Battery malfunction (low voltage) • Open circuit in wiring harness between power window main switch and power window subswitch • Power window initialization procedure error

Diagnostic Procedure

Step | Inspection | Action
--- | --- | ---
1 | • Inspect the door glass operation by operating the power window subswitch. • Does it operate normally? | Yes | Go to the next step.
No | Inspect the following parts, and repair or replace. • Power window subswitch (See POWER WINDOW SUBSWITCH INSPECTION.) • Power window motor (See POWER WINDOW MOTOR INSPECTION.) • Battery (Low voltage)
2 | • Inspect the door glass operation by operating the power window subswitch. • Does it operate in auto? | Yes | Inspect the wiring harness between the power window main switch and the power window subswitch. If there is any malfunction, repair or replace the applicable part.
No | Perform the power window initialization procedure. (See POWER WINDOW SYSTEM INITIALIZATION PROCEDURE.)