AUDIO UNIT CONSTRUCTION/OPERATION

id092000101600

Construction

• An audio unit with AM/FM tuner/MP3/WMA (Windows Media Audio)/AAC (Advanced Audio Coding) applicable CD player is assembled in the audio panel.

ac5jjn00000376

Terminal Layout and Signal

Audio unit

Terminal | Signal
--- | ---
| 1A | Front door speaker LH (+)
1B | B+
1C | Front door speaker LH (-)
1D | Front door speaker RH (+)
1E | TNS (+)
1F | Front door speaker RH (-)
1G | TNS (–)
1H | Steering switch 3
1I | Vehicle speed signal
1J | AMP control *1
1K | Parking brake signal
1L | —
1M | R position signal
1N | Steering switch 1
1O | CAN_H
1P | Steering switch 2
1Q | CAN_L
1R | ACC
1S | Rear door speaker LH (+)
1T | AudioPilot®2 *1
1U | Rear door speaker LH (-)
1V | Rear door speaker RH (+)
1W | Power ground
1X | Rear door speaker RH (-)
| 2A | Bluetooth signal input RH (+)
2B | Bluetooth signal input RH (-)
2C | Bluetooth signal input LH (+)
2D | Bluetooth signal input LH (-)
2E | Audio signal input RH (+)
2F | Audio signal input RH (-)
2G | Audio signal input LH (+)
2H | Audio signal input LH (-)
2I | HS-CAN (+)
2J | HS-CAN (-)
2L | Microphone voice input (+)
2N | Microphone voice input (-)
2P | Microphone ground
2R | Microphone power supply
2T | Microphone detect
2V | —
2W | AUX detection
2X | AUX signal LH, RH (-)
2Y | AUX signal RH (+)
2Z | AUX signal LH (+)
2AA | —
2AB | —
2AC | —
2AD | —
| 3A | Rear mount camera power supply
3B | Rear mount camera power supply ground
3C | Rear mount camera image ground
3D | Rear mount camera power signal input
| 4UA | USB power ground
4UB | USB data (+)
4UC | USB power supply
4UD | USB data (-)
| 5A | USB power supply
5B | USB data (+)
5C | USB power ground
5D | USB data (-)

*1 :With Bose®

Antenna feeder connector

Terminal | Signal
--- | ---
| 6A | ANT CONT
6B | Antenna

Switch location

With RDS (radio data system)

ac9wzn00000903

No. | Switch name | Function
--- | --- | ---
1 | EJECT button | Ejects CD.
2 | AUDIO button | Switches to audio screen.
3 | PHONE button | Switches to Bluetooth dial screen.
4 | NAV button | Switches to navigation screen.
5 | POWER/VOLUME button | Audio power on/off and volume adjustment are possible.
6 | SETUP button | Switches to setting screen.
7 | SEEK/TRACK button(up) | • Fast-forwards current tracks or radio stations. • Changes CD tracks or switches radio stations.
8 | SEEK/TRACK button(down) | • Reverses current tracks or radio stations. • Changes CD tracks or switches radio stations.
9 | TUNE/FILE AUDIO CONT button | • Changes CD tracks or switches radio stations. • Audio sound quality can be adjusted.

Without RDS (radio data system)

ac9wzn00000904

No. | Switch name | Function
--- | --- | ---
1 | EJECT button | Ejects CD.
2 | SETUP button | Switches to setting screen.
3 | SEEK/TRACK button(up) | • Fast-forwards current tracks or radio stations. • Changes CD tracks or switches radio stations.
4 | SEEK/TRACK button(down) | • Reverses current tracks or radio stations. • Changes CD tracks or switches radio stations.
5 | TUNE/FILE AUDIO CONT button | • Changes CD tracks or switches radio stations. • Audio sound quality can be adjusted.
6 | AUDIO button | Switches to audio screen.
7 | PHONE button | Switches to Bluetooth dial screen.
8 | NAV button | Switches to navigation screen.
9 | POWER/VOLUME button | Audio power on/off and volume adjustment are possible.