BRAKE FLUID LEVEL SENSOR INSPECTION

id041100801400

1. Disconnect the brake fluid level sensor connector from the master cylinder.

2. Inspect for continuity according to fluid level between the brake fluid level sensor terminals.

ac9uuw00001418

  • If not as indicated in the table, replace the No.1 reserve tank. (See MASTER CYLINDER REMOVAL/INSTALLATION [L.H.D.].) (See MASTER CYLINDER REMOVAL/INSTALLATION [R.H.D.].)

ac9wzw00003174