REAR WASHER HOSE REMOVAL/INSTALLATION

id091900801600

1. Disconnect the negative battery cable.

2. Remove the splash shield (RH). (See SPLASH SHIELD REMOVAL/INSTALLATION.)

3. Disconnect rear washer hose A from the washer tank.

ac9wzw00002609

4. Remove rear washer hose A from clip A, B.

5. Disconnect joint pipe A and remove rear washer hose A.

6. Disconnect joint pipe B and remove rear washer hose B.

7. Remove the grommet.

8. Remove the following parts:

  (1) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (3) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Dashboard under cover (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (6) Glove compartment service hole cover (See AIR FILTER REMOVAL/INSTALLATION.)

  (7) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

  (8) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (9) Console panel (See CONSOLE PANEL REMOVAL/INSTALLATION.)

  (10) Console cover (See CONSOLE COVER REMOVAL/INSTALLATION.)

  (11) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (12) Front scuff plate inner (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (13) Front side trim (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

  (14) Bonnet release lever (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION.)

  (15) Lower panel (See LOWER PANEL REMOVAL/INSTALLATION.)

  (16) Column cover (See COLUMN COVER REMOVAL/INSTALLATION.)

  (17) Driver-side air bag module (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

  (18) Steering wheel (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

  (19) Combination switch (See COMBINATION SWITCH REMOVAL/INSTALLATION.)

  (20) Center panel (See CENTER PANEL REMOVAL/INSTALLATION.)

  (21) Meter hood (See METER HOOD REMOVAL/INSTALLATION.)

  (22) Instrument cluster (See INSTRUMENT CLUSTER REMOVAL/INSTALLATION.)

  (23) Audio unit (vehicles with audio system) (See AUDIO UNIT REMOVAL/INSTALLATION.)

  (24) Car-navigation unit (vehicles with car-navigation system) (See CAR-NAVIGATION UNIT REMOVAL/INSTALLATION.)

  (25) Steering shaft (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

  (26) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)

  (27) Side panel (See SIDE PANEL REMOVAL/INSTALLATION.)

9. Disconnect joint pipe C and remove rear washer hose B.

10. Remove rear washer hose C from clips C.

11. Disconnect joint pipe D and remove rear washer hose C.

12. Remove the following parts:

  (1) Rear scuff plate inner (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (2) Front seat belt lower anchor installation bolt (Driver side) (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (3) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)

  (4) Front seat belt upper anchor installation bolt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (5) B-pillar upper trim (See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)

  (6) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (7) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (8) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (9) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (10) Third-row seat belt lower anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (11) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

  (12) Roof side trim (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)

  (13) Second-row seat belt upper anchor installation bolt (See SECOND-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (14) C-pillar trim (See C-PILLAR TRIM REMOVAL/INSTALLATION.)

  (15) Third-row seat belt upper anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (16) D-pillar trim (See D-PILLAR TRIM REMOVAL/INSTALLATION.)

  (17) Intruder sensor (vehicles with intruder sensor) (See INTRUDER SENSOR REMOVAL/INSTALLATION.)

  (18) Front map light (See FRONT MAP LIGHT REMOVAL/INSTALLATION.)

  (19) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)

  (20) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)

13. Disconnect joint pipe E and remove rear washer hose D.

ac9wzw00001598

14. Remove the headliner. (See HEADLINER REMOVAL/INSTALLATION.)

  Note
  • Rear washer hose C is integrated with the headliner. If rear washer hose C is to be replaced, replace it with the headliner as a single unit.

15. Remove rear washer hose E from the rear washer nozzle.

ac9wzw00002610

16. Install in the reverse order of removal.