REAR WASHER NOZZLE REMOVAL/INSTALLATION

id091900802200

1. Disconnect the negative battery cable.

2. Remove the liftgate upper trim. (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION.)

3. Remove the rear spoiler. (See REAR SPOILER REMOVAL/INSTALLATION.)

4. Press the tabs and remove the rear washer nozzle.

ac9wzw00001605

5. Install in the reverse order of removal.

6. Adjust the rear washer nozzle. (See REAR WASHER NOZZLE ADJUSTMENT.)