POWER WINDOW SYSTEM OUTLINE

id091200006400

• The following functions have been adopted for windows.

  ― Exterior open/close function (with exterior open/close)
  ― Manual open/close function
  ― Auto-open/close function (with auto-open/close)
  ― Auto reverse pinch protection function (with auto-open/close)
  ― Two-step down function (with auto-open/close)
  ― IG OFF timer function
  ― Fail-safe function

• A power-cut function that permits disabling the operation of all window switches from the driver‘s seat has been adopted.
• The P/W CM (power window control module) inside the power window switch, which detects the door glass movement distance and direction based on pulse signals of the power window motor, controls these functions.