PARKING SENSOR SWITCH/INDICATOR INSPECTION

id092200023800

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Dashboard under cover (Driver side) (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (2) Bonnet release lever (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION.)

  (3) Parking sensor switch/indicator (See PARKING SENSOR SWITCH/INDICATOR REMOVAL/INSTALLATION.)

3. Verify that the continuity is as indicated in the table.

ac9wzw00002629

  • If not as indicated in the table, replace the parking sensor switch/indicator.

ac9wzw00002630

4. Apply battery voltage to connect terminal H, and connect terminal J to ground.

5. Verify that the LED illuminates.

  • If there is any malfunction, replace the parking sensor switch/indicator.

6. Apply battery voltage to parking sensor switch terminal B, and connect terminal D to ground.

7. Verify that the LED illuminates.

  • If there is any malfunction, replace the parking sensor switch/indicator.