LIGHT SWITCH INSPECTION

id091800802900

1. Disconnect the negative battery cable.

2. Remove the lower column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

3. Remove the light switch. (See LIGHT SWITCH REMOVAL/INSTALLATION.)

4. Verify that the continuity between the light switch terminals is as indicated in the table.

Light Switch (LH) (Vehicle With Auto Light)

acxaaw00001111

• If not as indicated in the table, replace the light switch.

ac9wzw00001712

Turn switch

acxaaw00001011

acxuuw00001735

Light Switch (LH) (Vehicle without auto light)

ac9wzw00002635

• If not as indicated in the table, replace the light switch.

ac9wzw00002636

Turn switch

acxaaw00001011

acxuuw00001735

Light Switch (RH)

ac9wzw00001715

• If not as indicated in the table, replace the light switch.

ac9wzw00001716

Turn switch

am8rrw00001185

acxaaw00001167