PROPELLER SHAFT REMOVAL/INSTALLATION

id031500800300

1. Remove the presilencer installation nuts. (Middle pipe side) (See EXHAUST SYSTEM REMOVAL/INSTALLATION [MZI-3.7].)

2. Disconnect the hanger rubber as shown in the figure.

ac9uuw00002494

3. Suspend the presilencer using a cable.

4. Remove the presilencer insulator.

5. Remove in the order indicated in the figure.

6. Install in the reverse order of removal.

ac9wzw00000846

1 | Under guard (LH) (See CHARCOAL CANISTER, CANISTER VENT (CV) SOLENOID VALVE, AIR FILTER COMPONENT REMOVAL/INSTALLATION [MZI-3.7].)
2 | Member
3 | Nut (See Bolt and Nut Removal Note.)
4 | Bolt
5 | Bush
6 | Spacer
7 | Bolt (See Bolt and Nut Removal Note.)
8 | Propeller shaft (SeePropeller Shaft Installation Note.)

Bolt and Nut Removal Note

  Caution
  • Do not mark with a punch to prevent imbalance.

1. Before removing the nut, place alignment marks on the companion flange (front) and constant velocity joint, and on the companion flange (rear) and yoke.

acxuuw00001383

Propeller Shaft Installation Note

1. Align the alignment marks and install the propeller shaft.

acxuuw00001383

2. When installing a new propeller shaft, align the rear differential companion flange mark with the tag on the propeller shaft so that they are at the nearest position, and assemble.

ac9uuw00001399

3. Perform a road test and verify that there is no abnormal vibration or noise.