ADJUSTER ANCHOR REMOVAL/INSTALLATION

id081100802000

  Warning
  • Side air bag sensor No.1 is attached to the lower part of the B-pillar. When working around the B-pillar, disconnect the negative battery cable or work carefully, avoiding excessive impact to the lower part of the B-pillar.

1. Turn the ignition switch to the OFF position.

2. Disconnect the negative battery cable.

3. Remove the following parts:

  (1) Front scuff plate inner (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (2) Rear scuff plate inner (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (3) Front seat belt lower anchor installation bolt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (4) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)

  (5) Front seat belt upper anchor installation bolt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (6) B-pillar upper trim (See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)

4. Remove the bolt.

ac9wzw00000947

5. Rotate the adjuster anchor in the direction of the arrow.

6. Remove the adjuster anchor by pulling it outward.

7. Install in the reverse order of removal.