DTC B110E, B110F, B2856, B2886, B2887

id080200811800

DTC | B110E | Driver-side side air bag sensor No.2 ID mismatch
--- | --- | ---
B110F | Passenger-side side air bag sensor No.2 ID mismatch
B2856 | Crash zone sensor ID mismatch
B2886 | Passenger-side side air bag sensor No.1 ID mismatch
B2887 | Driver-side side air bag sensor No.1 ID mismatch
DETECTION CONDITION | Warning • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection according to only the detection conditions may cause injury due to an operating error, or damage the system. When performing an inspection, always follow the inspection procedure. • The SAS control module detects an error of impact magnitude set in the sensor, which occurs due to installation mismatch of the crash zone sensor or side air bag sensors.
POSSIBLE CAUSE | • Crash zone sensor misinstalled with wrong sensor • Driver-side side air bag sensor No.1 misinstalled with wrong sensor • Passenger-side side air bag sensor No.1 misinstalled with wrong sensor • Driver-side side air bag sensor No.2 misinstalled with wrong sensor • Passenger-side side air bag sensor No.2 misinstalled with wrong sensor

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT EACH SENSOR FOR INSTALLATION POSITION Warning • Handling the air bag system components improperly can accidentally deploy the air bag modules and pre-tensioner seat belts, which may seriously injure you. Read the service warnings and cautions before handling the air bag system components. (See AIR BAG SYSTEM SERVICE WARNINGS.) (See AIR BAG SYSTEM SERVICE CAUTIONS.) • Turn the ignition switch to the OFF position. • Disconnect the negative battery cable and wait for 1 min or more. • Verify that the crash zone sensor or side air bag sensor is installed in the correct position. • Is each sensor installed correctly? | Yes | Go to the next step.
No | Install the each sensor correctly, then go to the next step.
2 | INSPECT SAS CONTROL MODULE • Connect the negative battery cable. • Turn the ignition switch to the ON position. • Are DTCs B110E, B110F, B2856, B2886 and/or B2887 indicated? | Yes | Replace the SAS control module. (See SAS CONTROL MODULE REMOVAL/INSTALLATION.)
No | DTC troubleshooting completed.