ON-BOARD DIAGNOSTIC SYSTEM ACTIVE COMMAND MODES FUNCTION

id030200108500

• The active command modes function is used for optionally selecting active command modes items of input/output parts preset in the 4-wheel drive (4WD) control module (CM), and to operate them regardless of CM control.

Active Command Modes Table

Command name | Output part name | Operation | Operation condition
--- | --- | --- | ---
4WD_MODE | 4WD solenoid | OFF/ON | Ignition switch at ON