SELECTOR LEVER COMPONENT INSPECTION

id051800800600

1. Disconnect the negative battery cable.

2. Remove the center console.

3. Remove the dashboard completely. (See DASHBOARD REMOVAL/INSTALLATION.)

4. Disconnect the selector lever component connector.

5. Inspect for continuity at the selector lever component.

ac9uuw00002020

  • If there is any malfunction, adjust the selector cable. (See SELECTOR CABLE ADJUSTMENT.)

ac9uuw00002021