GENERAL PROCEDURES (STEERING)

id061000800100

Wheels and Tire Installation

1. When installing the wheels and tires, tighten the wheel nuts in a criss-cross pattern to the following tightening torque.

  Tightening torque

  107.8—147.0 N·m {11.0—14.9 kgf·m, 79.6—108.4 ft·lbf}

Connector Disconnection

1. Disconnect the negative battery cable before performing any work that requires handling of connectors. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

Power Steering Components Removal/Installation

1. If any power steering fluid line has been disconnected anytime during the procedure, add ATF M-III, M-V or Dexron®II, bleed the fluid lines, and inspect for leakage after the procedure has been completed.