DOOR SASH FILM INSTALLATION

id091600805300

1. Remove any grease or dirt from the affixing surface of the door.

2. Cut away the unused portion along the dotted lines.

acxuuw00000915

3. Peel off the backing paper and attach the door sash film onto the door as shown in the figure.

ac9uuw00000487

  Standard clearance

  a: 2.0 mm or more {0.08 in or more}
  b: 3.0—5.0 mm {0.12—0.19 in}

4. Peel off the transparent protective film on the door sash film.

5. Install the following parts:

  (1) Rear door garnish (See REAR DOOR GARNISH REMOVAL/INSTALLATION.)

  (2) Rear sash molding (See REAR SASH MOLDING INSTALLATION.)

  (3) Front sash molding (See FRONT SASH MOLDING INSTALLATION.)

  (4) Rear beltline molding (See REAR BELTLINE MOLDING REMOVAL/INSTALLATION.)

  (5) Front beltline molding (See FRONT BELTLINE MOLDING REMOVAL/INSTALLATION.)

  (6) Rear door trim (See REAR DOOR TRIM REMOVAL/INSTALLATION.)

  (7) Inner sail garnish (See INNER SAIL GARNISH REMOVAL/INSTALLATION.)

  (8) Front door trim (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

  (9) Inner garnish (See INNER GARNISH REMOVAL/INSTALLATION.)