FRONT CLIMATE CONTROL UNIT CONSTRUCTION

id074000105500

• A logic-type climate control unit is used with the full-auto air conditioner.
• The operation condition is displayed in the information display.
• When the DUAL switch is on, the airflow temperature for each side can be set using the driver and passenger-side temperature setting dials. If the DUAL switch is operated during the defroster mode, the mode does not change to the DUAL mode.
• When the ambient temperature switch is pressed, ambient temperature is displayed in the information display.
• When the ambient temperature switch is pressed approx. 3 s or more, the temperature setting display in the information display changes from °C to °F. (General (L.H.D.) specs.)
• When the rear control switch is on, the rear A/C can be operated using the rear climate control unit.
• A seat warmer switch is integrated. (See SEAT OUTLINE.)
• The rear window defroster switch is integrated. (See REAR WINDOW DEFROSTER FUNCTION OPERATION.)
• When the ambient temperature is 4 °C {39 °F}or less, the front climate control unit switches the display of the front passenger-side temperature setting to display of the ambient temperature in the information display, flashes the ambient temperature display, and sounds the buzzer to alert the driver.
The front climate control unit stops the ambient temperature warning control when the ambient temperature switch, DUAL switch, or the passenger-side temperature setting dial is operated. (General (L.H.D.) specs.)

L.H.D.

ac9wzn00000867

R.H.D.

ac9wzn00000529