NO.26 STARTER DOES NOT WORK [AY6A-EL, AY6AX-EL]

id0503k3803100

26 | Starter does not work
DESCRIPTION | • Starter does not work even when in P or N position.
POSSIBLE CAUSE | • Selector lever mis-adjustment • TR switch malfunction • N position learning is not performed. • Transaxle operates in fail-safe function (Starter lock system related circuit open or short) • Immobilizer system operating or system malfunction.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Perform the N position learning. (See TCM REMOVAL/INSTALLATION [AY6A-EL, AY6AX-EL].) • Does the problem eliminate? | Yes | Troubleshooting is completed. If the other symptom occurs, go to applicable troubleshooting procedure.
No | Go to the next step.
2 | • Inspect the TR switch. (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [AY6A-EL, AY6AX-EL].) • Is the TR switch normal? | Yes | Go to engine system troubleshooting No.3 “WILL NOT CRANK” troubleshooting procedure.
No | Replace the TR switch and perform initial learning procedure. (See NO.17 EXCESSIVE SHIFT SHOCK FROM N TO D OR N TO R POSITION [AY6A-EL, AY6AX-EL].)
3 | • Verify test results. ― If normal, return to the diagnostic index to service any additional symptoms. ― If malfunction remains, inspect the related Service Bulletins and/or On-line Repair Information and perform repair or diagnosis. • If the vehicle is repaired, troubleshooting completed. • If the vehicle is not repaired or additional diagnostic information is not available, replace the TCM.