NO. 6 INSTRUMENT CLUSTER ILLUMINATION DOES NOT ILLUMINATE [INSTRUMENT CLUSTER]

id0903d5807900

6 | Instrument cluster illumination does not illuminate
--- | ---
POSSIBLE CAUSE | • Instrument cluster malfunction • Connector or pin malfunction • Fuse malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Turn the ignition switch to the ON position. • Turn the light switch to the TNS position. • Does the instrument cluster illumination turn on? | Yes | Troubleshooting completed.
No | Go to the next step.
2 | • Does the non-illumination include the entire instrument cluster? | Yes | Go to the next step.
No | Replace the instrument cluster.
3 | • Inspect the METER, ROOM and ILLUMI fuse. • Are the fuses normal? | Yes | Go to the next step.
No | Replace the fuse. • If the fuse is melted, inspect the wiring harness for short to ground. Repair or replace the wiring harness, then replace the fuse.
4 | • Turn the ignition switch to the OFF position. • Inspect the instrument cluster connector terminals for poor connection (such as damaged/pulled-out pins, and corrosion). • Are the terminals normal? | Yes | Replace the instrument cluster.
No | Repair or replace the terminal.