INNER HANDLE REMOVAL/INSTALLATION

id091400803300

Front

1. Disconnect the negative battery cable.

2. Remove the inner garnish. (See INNER GARNISH REMOVAL/INSTALLATION.)

3. Remove the front door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

4. Disconnect the door lock switch connector.

ac9wzw00001073

5. Detach the cables from the inner handle and door lock knob.

6. Install in the reverse order of removal.

Rear

1. Disconnect the negative battery cable.

2. Remove the inner sail garnish. (See INNER SAIL GARNISH REMOVAL/INSTALLATION.)

3. Remove the rear door trim. (See REAR DOOR TRIM REMOVAL/INSTALLATION.)

4. Detach the cables from the inner handle and door lock knob.

ac9uuw00001158

5. Install in the reverse order of removal.