ROOF CARRIER BRACKET REMOVAL/INSTALLATION

id091600801700

1. Disconnect the negative battery cable.

2. Partially peel back the seaming welt.

3. Remove the following parts:

  (1) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)

  (2) Front scuff plate inner (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (3) Rear scuff plate inner (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (4) Front seat belt lower anchor installation bolt (Driver side) (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (5) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)

  (6) Front seat belt upper anchor installation bolt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (7) B-pillar upper trim (See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)

  (8) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (9) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (10) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (11) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (12) Third-row seat belt lower anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (13) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION)

  (14) Roof side trim (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)

  (15) Second-row seat belt upper anchor installation bolt (See SECOND-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (16) C-pillar trim (See C-PILLAR TRIM REMOVAL/INSTALLATION.)

  (17) Third-row seat belt upper anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (18) D-pillar trim (See D-PILLAR TRIM REMOVAL/INSTALLATION.)

  (19) Front map light (See FRONT MAP LIGHT REMOVAL/INSTALLATION.)

  (20) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)

  (21) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)

  (22) Headliner (See HEADLINER REMOVAL/INSTALLATION.)

4. Remove the nuts.

ac9uuw00000553

5. Remove the roof carrier bracket.

6. Install in the reverse order of removal.

  Note
  • Install the roof carrier bracket so that the arrow on it faces inward.