INSTRUMENTATION/DRIVER INFO. PERSONALIZATION FEATURES SETTING PROCEDURE

id092200889900

High Beam Control (HBC) System

  Note
  • The FSC records the personalization setting information and controls the system based on the recorded setting information (previous set value) when the ignition is switched ON. The recorded personalization setting information is cleared if the battery cable is disconnected.

1. Connect the M-MDS to the DLC-2.

2. After vehicle identification, select the following from the M-MDS initialization screen.

  (1) “Module programming“

  (2) “Programmable Parameters”

3. Select menu in the “FSC”.

4. Select an item name, and than select option.

Mazda Modular Diagnostic System (M-MDS) display | Function | Initial setting | Setting contents | Control unit
--- | --- | --- | --- | ---
High Beam Control. | The high beam control (HBC) system can be disabled. | ON | Not Adopted. / OFF / ON | FSC

Blind Spot Monitoring (BSM) System

1. Connect the M-MDS to the DLC-2.

2. After vehicle identification, select the following from the M-MDS initialization screen.

  (1) “Module programming“

  (2) “Programmable Parameters”

3. Select menu in the “Personality”.

4. Select an item name, and than select option.

Mazda Modular Diagnostic System (M-MDS) display | Function | Initial setting | Setting contents | Control unit
--- | --- | --- | --- | ---
BSM buzzer | The operation of BSM warning alarm can be turned off. | Enabled | Disabled / Enabled | BSM control module

Lane Departure Warning System (LDWS)/Forward Obstruction Warning (FOW) System

  Note
  • The personalization setting for the LDWS/FOW system is switched by pressing the FOW/LDWS switch. If the FOW/LDWS switch is not pressed during a period of approx. 5 s while performing the personalization setting, the system returns to the system-on (operational)/off (non-operational) screen.
  • The FSC records the personalization setting information and controls the system based on the recorded setting information (previous set value) when the ignition is switched ON. The recorded personalization setting information is cleared if the battery cable is disconnected.

• Switch using the following procedure:

ac9wzw00002843

LCD | Function | Initial setting | Setting contents | Control unit
--- | --- | --- | --- | ---
FOW LDWS | The operation of LDWS and FOW can be turned off. | FOW ON/LDWS ON | FOW ON/LDWS ON, FOW ON/LDWS OFF, FOW OFF/LDWS ON, FOW OFF/LDWS OFF | FSC
LDWS Vol. | The volume of the LDWS warning alarm can be changed. | Hi | Hi / Lo | FSC
LDWS Sens. | The warning operation sensitivity of the LDWS can be changed. | Lo | Hi / Lo | FSC
FOW Dist. | The warning operation distance of the FOW can be changed. | Near | Far / Near | FSC