INTRUDER SENSOR COVER REMOVAL/INSTALLATION

id091700910100

1. Using a tape-wrapped flathead screwdriver, press the tabs in the direction of the arrows (1) shown in the figure, and remove the intruder sensor cover in the direction of the arrow (2).

am6zzw00002776

2. Disconnect the intruder connector.

am6zzw00002714

3. Remove the intruder sensor component. (See Intruder Sensor Installation Note.)

am6zzw00001797

4. Install in the reverse order of removal.

Intruder Sensor Installation Note

1. Fit the intruder sensor from the intruder sensor cover bearing surface.

am6zzw00001800

2. Push the intruder sensor in the indication of the arrow, while lightly tighten the screw.

am6zzw00002777

3. Use the spark plug gauge, adjust the intruder sensor clearance from the intruder sensor cover 1.2 mm {0.047 in} or less.

am6zzw00002778

  Caution
  • If the space between the intruder sensor and intruder sensor cover exceeds 1.2 mm {0.047 in}, the detection function of the intruder sensor may be reduced or operate incorrectly.

4. Tighten the screw.

am6zzw00001803

5. Connect the connector.

am6zzw00001804