REAR AIR MIX ACTUATOR REMOVAL/INSTALLATION

id074000806000

1. Slide the passenger-side front seat to the maximum forward end.

2. Disconnect the negative battery cable.

3. Remove the following parts:

  (1) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (3) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Dashboard under cover (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (6) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (7) Console panel (See CONSOLE PANEL REMOVAL/INSTALLATION.)

  (8) Console cover (See CONSOLE COVER REMOVAL/INSTALLATION.)

  (9) Console (See CONSOLE REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

ac9wzw00002820

1 | Rear air mix actuator connector
2 | Screw
3 | Rear air mix actuator

5. Install in the reverse order of removal.