DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)]

id0902j3845800

HS-CAN

DTC output module (M-MDS display) | DTC | Malfunction location | Reference for inspection procedure
--- | --- | --- | ---
PCM (PCM) | U0101 | Communication error to TCM | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0140 | Communication error to BCM
TCM (TCM) | U0073:00*1 | CAN system communication error | (See DTC U0001:88, U0073, U0073:00 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0100:00 | Communication error to PCM | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0121:00 | Communication error to DSC/RSC HU/CM
U0155:00 | Communication error to instrument cluster
U0415:00*1 | Abnormal message from DSC/RSC HU/CM | (See DTC U0415:00 [AY6A-EL, AY6AX-EL].)
DSC/RSC HU/CM (ABS) | U0073*1 | CAN system communication error | (See DTC U0001:88, U0073, U0073:00 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0100 | Communication error to PCM | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0140 | Communication error to BCM
U0155 | Communication error to instrument cluster
BCM (GEM) | U0073*1 | CAN system communication error | (See DTC U0001:88, U0073, U0073:00 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0100 | Communication error to PCM | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0101 | Communication error to TCM
U0121 | Communication error to DSC/RSC HU/CM
U0401*1 | Abnormal message from PCM | (See DTC U0401 [BCM].)
4WD control module*2 (4×4) | U0073*1 | CAN system communication error | (See DTC U0001:88, U0073, U0073:00 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0100 | Communication error to PCM | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0101 | Communication error to TCM
U0121 | Communication error to DSC/RSC HU/CM
U0155 | Communication error to instrument cluster
Keyless control module*3 (RKE) | U0073*1 | CAN system communication error | (See DTC U0001:88, U0073, U0073:00 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0100 | Communication error to PCM | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0140 | Communication error to BCM
U0323 | Communication error to instrument cluster
U2023*1 | Abnormal message from PCM | (See DTC U2023 [ADVANCED KEYLESS ENTRY AND START SYSTEM].)
PLG control module*4 (LTM) | U0073*1 | CAN system communication error | (See DTC U0001:88, U0073, U0073:00 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0100 | Communication error to PCM | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0101 | Communication error to TCM
U0140 | Communication error to BCM
U0155 | Communication error to instrument cluster
U0214 | Communication error to keyless control module
BSM control module (LH)*5 (BSML) | U0001:88*1 | CAN system communication error | (See DTC U0001:88, U0073, U0073:00 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0100:00 | Communication error to PCM | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0101:00 | Communication error to TCM
U0140:00 | Communication error to BCM
U0233:00 | Communication error to BSM control module (RH)
U0401:68*1 | Signal error from PCM | (See DTC U0401:68 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
U0402:68*1 | Signal error from TCM | (See DTC U0402:68 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
U0422:68*1 | Signal error from BCM | (See DTC U0422:68 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
U0534:68*1 | Signal error from BSM control module (RH) | (See DTC U0534:68 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
BSM control module (RH)*5 (BSMR) | U0001:88*1 | CAN system communication error | (See DTC U0001:88, U0073, U0073:00 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0100:00 | Communication error to PCM | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0101:00 | Communication error to TCM
U0140:00 | Communication error to BCM
U0232:00 | Communication error to BSM control module (LH)
U0401:68*1 | Signal error from PCM | (See DTC U0401:68 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
U0402:68*1 | Signal error from TCM | (See DTC U0402:68 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
U0422:68*1 | Signal error from BCM | (See DTC U0422:68 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
U0533:68*1 | Signal error from BSM control module (LH) | (See DTC U0533:68 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
Position memory control module*6 (DSM) | U0001:88*1 | CAN system communication error | (See DTC U0001:88, U0073, U0073:00 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0100:00 | Communication error to PCM | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0101:00 | Communication error to TCM
U0121:00 | Communication error to DSC/RSC HU/CM
U0140:00 | Communication error to BCM
U0155:00 | Communication error to instrument cluster
U0431:68*1 | Abnormal message from BCM | (See DTC U0431:68 [POSITION MEMORY CONTROL SYSTEM].)
SAS control module (RCM) | U0073*1 | CAN system communication error | (See DTC U0001:88, U0073, U0073:00 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0155 | Communication error to instrument cluster | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
Theft-deterrent control module*7 (VSM) | U0001:88*1 | CAN system communication error | (See DTC U0001:88, U0073, U0073:00 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0100:00 | Communication error to PCM | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0140:00 | Communication error to BCM
Forward sensing camera*8 (FSC) | U0001:88*1 | CAN system communication error | (See DTC U0001:88, U0073, U0073:00 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0100:00 | Communication error to PCM | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0121:00 | Communication error to DSC/RSC HU/CM
U0140:00 | Communication error to BCM
U0155:00 | Communication error to instrument cluster
U0401:68*1 | Abnormal message from PCM | (See DTC U0401:68 [FORWARD SENSING CAMERA (FSC)].)
U0415:68*1 | Abnormal message from DSC/RSC HU/CM | (See DTC U0415:68 [FORWARD SENSING CAMERA (FSC)].)
U0422:68*1 | Abnormal message from BCM | (See DTC U0422:68 [FORWARD SENSING CAMERA (FSC)].)
U0423:68*1 | Abnormal message from instrument cluster | (See DTC U0423:68 [FORWARD SENSING CAMERA (FSC)].)
U2005:86*1 | Abnormal message from PCM | (See DTC U2005:86 [FORWARD SENSING CAMERA (FSC)].)
Instrument cluster (IC) | U0073*1 | CAN system communication error | (See DTC U0001:88, U0073, U0073:00 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0100 | Communication error to PCM | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0101 | Communication error to TCM
U0114 | Communication error to 4WD control module
U0121 | Communication error to DSC/RSC HU/CM
U0140 | Communication error to BCM
U0151 | Communication error to SAS control module
U0200 | Communication error to BSM control module (RH)
U0214 | Communication error to keyless control module
U023A | Communication error to forward sensing camera
U2510*1 | Communication error to PCM | (See SECURITY LIGHT: 16, DTC: U2510/P1260/P1260:00 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)

*1 :If only the target DTCs are displayed, perform the corresponding DTC inspection without determining the open circuit location.
*2 :With 4WD
*3 :With advanced keyless entry and start system
*4 :With PLG system
*5 :With blind spot monitoring (BSM) control module connector 8-pin type
*6 :With memory power seat
*7 :With theft-deterrent system
*8 :With forward sensing camera

MS-CAN

DTC output module (M-MDS display) | DTC | Malfunction location | Reference for inspection procedure
--- | --- | --- | ---
Instrument cluster (IC) | U0200*2 | Communication error to BSM control module (LH) | (See DTC U0010:88, 01:Er, 01Er, 16:Er12 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
Audio unit (ACU) | U0010:88*1 (16:Er12) | CAN system communication error | (See DTC U0010:88, 01:Er, 01Er, 16:Er12 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
BSM control module (LH)*2 (BSML) | U0010:88*1 | CAN system communication error | (See DTC U0010:88, 01:Er, 01Er, 16:Er12 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0100:00 | Communication error to PCM | (See DETERMINING MALFUNCTIONING PART (MS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0140:00 | Communication error to BCM
Information display*3 | 01:Er*1 | CAN system communication error | (See DTC U0010:88, 01:Er, 01Er, 16:Er12 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
02:1E | Communication error to audio unit | (See DETERMINING MALFUNCTIONING PART (MS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
02:3E | Communication error to instrument cluster
Information display*4 | 01Er*1 | CAN system communication error | (See DTC U0010:88, 01:Er, 01Er, 16:Er12 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
02 1E | Communication error to audio unit | (See DETERMINING MALFUNCTIONING PART (MS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
02 3E | Communication error to instrument cluster

*1 :If only the target DTCs are displayed, perform the corresponding DTC inspection without determining the open circuit location.
*2 :With blind spot monitoring (BSM) control module connector 10-pin type
*3 :With clock display
*4 :Without clock display