Bose ADAPTER REMOVAL/INSTALLATION

id092000815300

1. Disconnect the negative battery cable.

2. Remove the dashboard under cover (Driver side). (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

3. Disconnect the connector.

ac9wzw00002906

4. Remove the nuts.

5. Remove in the Bose® adapter.

6. While pressing the tabs of the clip in the direction of arrows (1) shown in the figure, press the clip in the direction of arrow (2) to detach it from the Bose.adapter.

ac9wzw00002907

7. Remove the clip.

8. Disconnect the connector.

9. Remove the screws.

ac9wzw00002908

10. Remove the Bose® adapter from the bracket.

11. Install in the reverse order of removal.