B-PILLAR LOWER TRIM REMOVAL/INSTALLATION

id091700802000

1. Remove the front scuff plate inner. (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

2. Remove the rear scuff plate inner. (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

3. Remove the front seat belt lower anchor installation bolt. (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

4. Partially peel back the seaming welt.

ac9uuw00000329

5. Detach tabs A and clips B and D, and pins C, by pulling them in the direction of the arrow.

6. Remove the B-pillar lower trim.

7. Install in the reverse order of removal.