A-PILLAR TRIM REMOVAL/INSTALLATION

id091700801900

1. Partially peel back the seaming welt.

2. Pull the A-pillar trim shown in the figure in the direction of the arrow, raise clip B from its grommet together with the A-pillar trim, and remove clips A at the same time.

ac9uuw00002639

3. Slide the A-pillar trim in the direction of the arrow shown in the figure and remove the A-pillar trim from clip B.

ac9uuw00002640

4. Rotate and pull the clip B in the direction of the arrow shown in the figure until it is no longer loose, and feels tight.

ac9uuw00002635

5. Pull the clip B and remove it from the grommet.

6. Insert a tape-wrapped flathead screwdriver between the body and the grommet.

ac9wzw00003020

7. Press the tabs and remove the grommet.

8. Install the new grommet to the body.

9. Install the new clip B to the A-pillar trim.

10. Install the A-pillar trim.