PURGE SOLENOID VALVE CONSTRUCTION/OPERATION [MZI-3.7]

id0116d2102400

• Opens and closes the valve according to the purge solenoid valve control signal (duty signal) from the PCM to control the amount of evaporative gas to be introduced to the dynamic chamber according to engine operation conditions.
• The passage between the ports opens when the PCM sent the signal, and evaporative gas is introduced to the intake air system according to intake manifold vacuum.

ac9wzn00000539