ON-BOARD DIAGNOSTIC SYSTEM PID/DATA MONITOR FUNCTION

id030200108400

• The parameter identification (PID)/data monitor function is used for optionally selecting input/output signal monitor items preset in the 4-wheel drive (4WD) control module (CM) and reading them out in real-time.

PID/DATA Monitor Table

PID/data monitor item | Input/output part | Unit/Condition (Tester display)
--- | --- | ---
AAT | Ambient air temperature | °C/°F
APP | Accelerator pedal position | %
BOO | Brake ON/OFF | OFF/ON
COUP_SOL | Coupling solenoid duty cycle | %
OIL_TEMP | Rear differential oil temperature | °C/°F
OIL_TEMP | Rear differential oil temperature | V
VPWR | Ignition voltage | V
WSPD_LF | ABS wheel-speed sensor (LF) | KPH, MPH
WSPD_LR | ABS wheel-speed sensor (LR) | KPH, MPH
WSPD_RF | ABS wheel-speed sensor (RF) | KPH, MPH
WSPD_RR | ABS wheel-speed sensor (RR) | KPH, MPH
4WD_LAMP | 4WD mode lamp | OFF/BLINK/ON