REAR DOOR TRIM REMOVAL/INSTALLATION

id091700802600

1. Disconnect the negative battery cable.

2. Remove the inner sail garnish. (See INNER SAIL GARNISH REMOVAL/INSTALLATION.)

3. Open the cover A using a small flathead screwdriver and remove the screw.

4. Pull up the cover B and remove the screw.

ac9uuw00000489

5. Detach clips A from the front door using a fastener remover.

6. Pull the front door trim upward and detach tabs B from the front door.

7. Remove tab A, and move the rear door trim in the direction of the arrow.

ac9uuw00002107

8. Turn the inner handle cover in the direction of the arrow and remove it from the rear door trim.

ac9uuw00002108

9. Disconnect the power window subswitch connector.

10. Remove the rear door trim.

11. Install in the reverse order of removal.