SLIDE MOTOR INSPECTION

id091300800900

1. Disconnect the slide motor connector.

2. Apply battery positive voltage to the slide motor terminals and inspect the slide motor operation

ac9wzw00001244

  • If not as specified, replace the slide adjuster. (See FRONT SEAT SLIDE ADJUSTER REMOVAL/INSTALLATION.)

Motor operation | Connection
--- | ---
B+ | GND
Forward | 2A | 2B
Backward | 2B | 2A

3. Connect the slide motor connector.

4. Measure the slide motor terminal 1C waveform during motor operation using the oscilloscope.

Condition | Voltage (V)
--- | ---
High output | 4.8 or more
Low output | 1.0 or less

• If not as specified, replace the slide adjuster. (See FRONT SEAT SLIDE ADJUSTER REMOVAL/INSTALLATION.)