PURGE SOLENOID VALVE INSPECTION [MZI-3.7]

id0116d2800900

Airflow Inspection

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

2. Disconnect the quick release connector from the purge solenoid valve. (See QUICK RELEASE CONNECTOR (EMISSION SYSTEM) REMOVAL/INSTALLATION [MZI-3.7].)

3. Remove the purge solenoid valve. (See PURGE SOLENOID VALVE REMOVAL/INSTALLATION [MZI-3.7].)

4. Verify that the airflow is as indicated in the table.

ac9wzw00001558

Measured condition | Continuity between A—B
--- | ---
When voltage is not applied between terminals A and B | No airflow
When voltage is applied between terminals A and B | Airflow detected

  • If not as specified in the table, inspect the purge solenoid valve. (See PURGE SOLENOID VALVE REMOVAL/INSTALLATION [MZI-3.7].)