HEADLIGHT CLEANER ACTUATOR REMOVAL/INSTALLATION

id091900803000

1. Disconnect the negative battery cable.

2. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Remove the headlight cleaner nozzle cover.

ac9wzw00003024

4. Disconnect headlight cleaner hose from the headlight cleaner actuator.

5. Remove the headlight cleaner actuator.

6. Install in the reverse order of removal.