FRONT WHEEL HUB BOLT REPLACEMENT

id031100800200

1. Remove the brake calliper component from the steering knuckle and suspend it out of the way using a cable.

2. Remove the disc plate.

3. Tap the dust cover (the part shown in the figure) with a chisel lightly and bend the processing point back to the steering knuckle side.

ac9wzw00000048

4. Remove the wheel hub bolt using the SST as shown in the figure.

ac9wzw00000049

5. Place a new wheel hub bolt in the wheel hub.

6. Install the wheel hub by placing a proper sized washer on the hub, and tightening the nut as shown in the figure.

ac9wzw00000050