DTC P2127:00 [MZI-3.7]

id0102d2708500

DTC P2127:00 | APP sensor No.2 circuit low input
--- | ---
DETECTION CONDITION | • APP sensor No.2 is out of self-test range low.
POSSIBLE CAUSE | • Connector or terminal malfunction • Short to ground circuit between APP sensor terminal F and PCM terminal 1X • Short to ground circuit between APP sensor terminal A and PCM terminal 1Z • Short to ground circuit between APP sensor terminal D and PCM terminal 1AB • Short to ground circuit between APP sensor terminal C and PCM terminal 1AD • Short to ground circuit between APP sensor terminal B and PCM terminal 1U • APP sensor malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED SERVICE INFORMATION AVAILABILITY • Verify related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to the available Service Information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT APP SENSOR CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect the APP sensor connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Are there any malfunction? | Yes | Repair or replace suspected part, then go to Step 7.
No | Go to the next step.
4 | INSPECT APP SENSOR NO.2 CIRCUIT FOR SHORT TO GROUND • APP sensor connector is disconnected. • Turn the ignition switch off. • Inspect for continuity between the following terminals: ― APP sensor terminal F (wiring harness-side) and body ground. ― APP sensor terminal A (wiring harness-side) and body ground. ― APP sensor terminal D (wiring harness-side) and body ground. ― APP sensor terminal C (wiring harness-side) and body ground. ― APP sensor terminal B (wiring harness-side) and body ground. • Are there continuity? | Yes | Repair or replace suspected part, then go to Step 7.
No | Go to the next step.
5 | INSPECT APP SENSOR NO.2 • Inspect APP sensor No.2. (See ACCELERATOR PEDAL POSITION (APP) SENSOR INSPECTION [MZI-3.7].) • Is there any malfunction? | Yes | Replace the accelerator pedal, then go to Step 7. (See ACCELERATOR PEDAL REMOVAL/INSTALLATION [MZI-3.7].)
No | Go to the next step.
6 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect the PCM connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Are there any malfunction? | Yes | Repair or replace suspected part, then go to Step 7.
No | Go to the next step.
7 | VERIFY TROUBLESHOOTING OF DTC P2127:00 HAS BEEN COMPLETED • Verify that all disconnected connectors reconnected. • Clear the DTC from the PCM memory using the M-MDS. • Start the engine. • Is the same DTC present? | Yes | Repeat the inspection from Step 1. • If the malfunction recurs, replace the PCM. (See PCM REMOVAL/INSTALLATION [MZI-3.7].) Go to the next step.
No | Go to the next step.
8 | VERIFY AFTER REPAIR PROCEDURE • Perform the “AFTER REPAIR PROCEDURE”. (See AFTER REPAIR PROCEDURE [MZI-3.7].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [MZI-3.7].)
No | Troubleshooting completed.