REAR BRAKE (DISC) REMOVAL/INSTALLATION

id041100800500

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

3. After installation, add brake fluid, bleed the air, and inspect for fluid leakage. (See AIR BLEEDING.)

4. After installation, do the following.

  (1) Depress the brake pedal a few times. Then verify that the brakes do not drag.

  (2) Inspect the parking brake pedal stroke. (See PARKING BRAKE INSPECTION.)

ac9wzw00000138

1 | Brake hose
2 | Bolt
3 | Caliper (See Caliper Installation Note.)
4 | Disc pad
5 | Shim
6 | Guide plate
7 | Bolt
8 | Mounting support
9 | Slide pin
10 | Bush
11 | Dust boot
12 | Plug
13 | Screw (See Disc Plate, Screw Installation Note.)
14 | Disc plate (See Disc Plate Removal Note.) (See Disc Plate, Screw Installation Note.)

Disc Plate Removal Note

1. If any disc plate is difficult to remove, perform the following steps to remove it.

  (1) Insert a flathead screwdriver into the service hole and turn the adjuster in the direction of the arrow to compress the parking brake shoe.

  ac9uuw00001434

  (2) Remove the disc plate.

Disc Plate, Screw Installation Note

1. Install the disc plate and the screws.

2. Perform the following steps to adjust the shoe clearance after installing the disc plate and the screws.

  (1) Insert a flathead screwdriver into the service hole and turn the adjuster in the direction of the arrow to expand the parking brake shoe until the disc plate cannot rotate.

  ac9uuw00001435

  (2) Return the adjuster 13—25 notches in the direction of the arrow.

  ac9uuw00001436

    Note
    • Shoe clearance can be adjusted to 0.15 mm {0.006 in} by returning the adjuster 15 notches.

  (3) Rotate the disc plate and make sure it does not drag.

Caliper Installation Note

1. Push the piston fully inward using the SST.

2. Install the caliper.

ac9uuw00001437