FOW/LDWS SWITCH

id092200035300

Purpose

• The lane departure warning system (LDWS) and forward obstruction warning (FOW) system can be turned on or off optionally by the driver.

Function

• The switch operation signal is sent to the instrument cluster.

Construction

• The FOW/LDWS switch is built into the cluster switch.

ac9wzn00000802

Operation

1. When the FOW/LDWS switch operates, the switch operation signal is sent to the instrument cluster.
2. When the instrument cluster receives the switch operation signal from the cluster switch, and the switch operation signal is sent to the FSC.
3. When the FSC receives the switch operation signal from the instrument cluster, it switches the FOW/LDWS on/off.

ac9wzn00000803

Fail-safe

• Function not equipped.