PCM CONFIGURATION [MZI-3.7]

id0140c3802600

  Note
  • Use the IDS (laptop PC) because the PDS (Pocket PC) does not support the PCM CONFIGURATION.

1. Connect the M-MDS to DLC-2.

ac9wzw00002366

2. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  • When using the IDS (laptop PC)
    1. Select the “Module Programming”.

3. Then, select the “Programmable Module Installation”, “PCM” from the screen menu.

4. Select “PCM” and perform procedures according to directions on the M-MDS screen.

5. Retrieve DTCs by the M-MDS, then verify that there is no DTC present.

  • If a DTC(s) is detected, perform the applicable DTC inspection. (See DTC TABLE [MZI-3.7].)