THEFT-DETERRENT SYSTEM OPERATION [WITHOUT INTRUDER SENSOR]

id0914005994b8

Operation

Mode transition

  • The BCM switches the theft-deterrent system mode based on the ignition switch and door conditions.

  ac9wzn00000966

Operation Stop Mode

• In this mode, all theft-deterrent system operations are stopped.
• The system changes to the operation stop mode when any of the following conditions are met.

  ― Ignition switch to the ON position
  ― Key reminder switch on
  ― Push switch on (with advanced keyless entry and start system)

Initial Mode

• This mode is the preparatory mode before changing to the stand-by mode. The system does not change directly to the alert mode from this mode.
Transition condition to the initial mode
• The system changes from the operation stop mode to the initial mode if all of the following conditions are met.

  ― Ignition switch to the OFF position
  ― Key reminder switch off
  ― Push switch off (with advanced keyless entry and start system)

• The system transitions from stand-by preparatory mode, stand-by mode, alert mode, and alert preparatory mode to the initial mode if the cancel conditions in each mode are met.
Transition condition to the stand-by preparatory mode
• The system changes to the stand-by preparatory mode if any of the following conditions are met.

  ― A lock operation was performed using the transmitter/advanced key lock button or key with all the doors, liftgate, and bonnet closed.

Stand-by Preparatory Mode

• This is mode prior to the stand-by mode.
• If the cancel conditions are met, the system changes to the initial mode.
Transition condition to the stand-by mode
• If the stand-by preparatory mode continues for approx. 20 s, the system changes to the stand-by mode.
Cancel conditions
• If any of the following conditions are met, the stand-by preparation mode is canceled and the system changes to the initial mode.

  ― The driver-side door key cylinder is unlocked
  ― Any door switch on (door is open), or liftgate latch switch on (liftgate is open), or bonnet latch switch off (bonnet is open)
  ― Any door lock-link switch UNLOCK
  ― Key reminder switch on, Ignition switch to the ON position, and engine start
  ― Unlock operation using transmitter/advanced key

Stand-by Mode

• The system starts monitoring approx. 20 s after the doors are locked for unauthorized door opening/closing, or movement from an intrusion into the vehicle such as a window being broken. If any unauthorized operation is detected, the system changes to the alert mode.
• If the cancel conditions are met, the system changes to the initial mode.
Transition condition to the alert mode
• If any of the following conditions are met, the system changes to the alert mode.

  ― Ignition switch to the ON position (key reminder switch off)
  ― Push switch off (with advanced keyless entry and start system)
  ― Any door switch on (door is open)
  ― Liftgate latch switch on (liftgate is open)
  ― Bonnet latch switch off (bonnet is open)
  ― Door lock-link switch UNLOCK

Cancel condition
• If any of the following conditions are met, the stand-by mode is canceled and the system changes to the initial mode.

  ― Key reminder switch on, Ignition switch to the ON position, and engine start
  ― Unlock operation using transmitter/advanced key
  ― The driver-side door key cylinder is unlocked

Alert Mode

• In this mode, the horn and hazard warning lights are operated to alert the surrounding area.
• When the alarm period (approx. 30 s) has elapsed, the system changes to the alert preparatory mode.
• If the cancel conditions are met, the system changes to the initial mode.

am5ezn00001783

Transition condition to the alert preparatory mode
• When the alarm period (approx. 30 s) has elapsed, the system changes to the alert preparatory mode.
• The alarm period is not extended even if a transition condition to alert mode is met again during an alarm period.
Cancel condition
• If any of the following conditions are met, the alert mode is canceled, and the system changes to the initial mode.

  ― Key reminder switch on, Ignition switch to the ON position, and engine start
  ― Unlock operation using transmitter/advanced key
  ― The driver-side door key cylinder is unlocked

Alert Preparatory Mode

• In the alert preparatory mode, the horn and hazard warning light are not operated, however, the alarm triggers immediately if the condition is changed.
• If the cancel conditions are met, the system changes to the initial mode.
Transition condition to alert mode
• The system changes to the alert mode if any of the following conditions are met.

  ― Ignition switch to the ON position (key reminder switch off)
  ― Push switch off (with advanced keyless entry and start system)
  ― Any door switch on (door is open)
  ― Liftgate latch switch on (liftgate is open)
  ― Bonnet latch switch off (bonnet is open)
  ― Door lock-link switch UNLOCK

Cancel condition
• If any of the following conditions are met, the alert preparatory mode is canceled and the system changes to the initial mode.

  ― Key reminder switch on, Ignition switch to the ON position, and engine start
  ― Unlock operation using transmitter/advanced key
  ― The driver-side door key cylinder is unlocked